{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Prio"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Prio","index":0,"n_rows":186,"n_cols":6,"rows_kept":186,"cut":false,"hidden":false,"merged":[]}
["Prioritätsliste / Liste des priorités (Attribut / attribut \"Prio\"):"]
["Üverarbeitung / révision : "]
["0= wird von swisstopo gemacht / sera effectuée par swisstopo"]
["1= prioritär (obligatorisch) / prioritaire (obligatoire)"]
["2= passiv (fakultativ) / passive (facultative)"]
["3= nicht prioritär; Drittdaten / non prioritaire; données tiers"]
[]
["Thema","Klasse","GeolCode","Objekt (KIND DE)","Objekt (KIND FR)","Prio"]
["Hydrogeology","Surface_Water_PLG",12701001,"Gletscher","glacier",0]
["Hydrogeology","Surface_Water_PLG",12701002,"See","lac",0]
["Hydrogeology","Surface_Water_PLG",12701003,"Fluss","rivière",0]
["Local Additional Informations","Geological_Outlines_L",13001001,"geologische Kontur","contour géologique",0]
["Local Additional Informations","Type_Localities_PT",13501003,"Typusprofil","coupe-type",0]
["Geomorphology","Erosional_Structures_L",11101001,"Erosionsrand","bord d´érosion",1]
["Geomorphology","Erosional_Structures_L",11101002,"Terrassenkante","bord de terrasse",1]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301001,"Moränenwall","vallum morainique",1]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301002,"Moränenwall auf Gletscher oder auf Toteis","cordon morainique sur glacier ou sur glace morte",1]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301003,"Kameterrassenkante","bord de terrasse de kame",1]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301006,"Protalus Rampart Wulst","bourrelet de protalus rampart",1]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301007,"Blockwulst im Blockgletscher","bourrelet de glacier rocheux",1]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301008,"Schneehaldenmoränenwall","vallum de moraine de névé",1]
["Geomorphology","Glacial_Structures_PLG",11401001,"Drumlin, drumlinartige Kieskuppe","drumlin, croupe graveleuse en forme de drumlin",1]
["Geomorphology","Glacial_Structures_PLG",11401003,"Rundhöcker","roches moutonnées",1]
["Geomorphology","Instabilities_PLG",15801001,"Sackungsgebiet","zone de tassement",1]
["Geomorphology","Instabilities_PLG",15801002,"Gebiet mit Hakenwurf","zone de fauchage",1]
["Geomorphology","Instabilities_PLG",15801003,"Rutschgebiet","zone de glissement",1]
["Geomorphology","Instabilities_PLG",15801004,"Gebiet mit Solifluktion","zone de solifluxion",1]
["Geomorphology","Instability_Structures_L",11701002,"Nackentälchen, Zerrstruktur","limite de contrepente, fente ouverte",1]
["Geomorphology","Instability_Structures_L",11701003,"Abrissrand","niche d´arrachement",1]
["Geomorphology","Instability_Structures_L",11701004,"offene Spalte","crevasse",1]
["Geomorphology","Instability_Structures_PT",11601001,"Hinweis auf Hanginstabilität","indice d'instabilité",1]
["Local Additional Informations","Artificial_Surface_Modifications_PLG",10401003,"Aufschüttung, Damm","remblai, digue",1]
["Local Additional Informations","Artificial_Surface_Modifications_PLG",10401004,"Auffüllung","remplissage",1]
["Local Additional Informations","Miscellaneous_PT",15501001,"Diverse","Divers",1]
["Local Additional Informations","Prominent_Lithological_Features_L",13101001,"Gesteinshorizont","horizon de roche",1]
["Measurements Spatial Orientation","Planar_Structures_PT",13801001,"Orientierung der Schichten","orientation des couches",1]
["Measurements Spatial Orientation","Planar_Structures_PT",13801004,"Orientierung der Schieferung","orientation d'une schistosité",1]
["Measurements Spatial Orientation","Planar_Structures_PT",13801005,"Orientierung einer Schichtung oder Schieferung","orientation d'une couche ou d'une schistosité",1]
["Rock Bodies","Bedrock_PLG",14334001,"Fesgestein","Roche en place",1]
["Rock Bodies","Unconsolidated_Deposits_PLG",14517001,"Lockergestein","roche meuble",1]
["Tectonics","Tectonic_Boundaries_L",14901001,"Überschiebung","chevauchement",1]
["Tectonics","Tectonic_Boundaries_L",14901002,"Abschiebung","détachement (faille normale de grande extension et faible pendage)",1]
["Tectonics","Tectonic_Boundaries_L",14901004,"Bruch","faille",1]
["Geomorphology","Alluvial_and_Lacustrine_Structures_L",10901002,"Achse einer Murgangrinne","axe d'un chenal de lave torrentielle",2]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301004,"älterer Gletscherstand, basierend auf historischen Daten","ancien stade glaciaire, déduit de données historiques",2]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301009,"Verbreitungsgrenze von alpinem Geschiebe","limite de l'étendue des blocs",2]
["Geomorphology","Glacial_Structures_PLG",11401004,"Toteisloch, Söll","doline glaciaire, kettle",2]
["Geomorphology","Glacial_Structures_PT",11201002,"Gletschermühle, Strudelloch","marmite glaciaire, cavité d´érosion",2]
["Geomorphology","Instability_Structures_L",11701001,"Stauchwulst","bourrelet de glissement",2]
["Geomorphology","Karstic_Structures_PLG",12001001,"Senke ohne oberirdischen Abfluss","dépression sans exutoire superficiel",2]
["Geomorphology","Karstic_Structures_PLG",12001002,"Doline","doline",2]
["Geomorphology","Karstic_Structures_PLG",12001003,"Karrenfeld","lapiez",2]
["Geomorphology","Karstic_Structures_PLG",12001004,"Polje","poljé",2]
["Geomorphology","Karstic_Structures_PT",11901001,"Ponor","ponor",2]
["Hydrogeology","Palaeohydrology_L",12301001,"Paläotal","axe de paléovallée",2]
["Hydrogeology","Palaeohydrology_L",12301002,"ehemalige Entwässerungsrinne","ancien chenal",2]
["Hydrogeology","Palaeohydrology_L",12301003,"glaziale Abflussrinne","axe d'un ancien effluent glaciaire",2]
["Hydrogeology","Palaeohydrology_L",12301004,"Trockental","vallée sèche",2]
["Hydrogeology","Palaeohydrology_L",12301005,"ehemaliges Bachbett","ancien lit d'un cours d'eau (ruisseau)",2]
["Hydrogeology","Palaeohydrology_L",12301006,"Ufer eines ehemaligen Flussbetts","rive d'un ancien lit d'un cours d'eau",2]
["Hydrogeology","Palaeohydrology_L",12301007,"ehemalige Uferlinie","ancienne ligne de rivage",2]
["Hydrogeology","Surface_Water_L",12601001,"Quellhorizont","niveau de sources, déversement de la nappe phréatique",2]
["Hydrogeology","Surface_Water_PT",12501002,"diffuse Quelle","source diffuse",2]
["Hydrogeology","Surface_Water_PT",12501003,"Wiederaustritt eines unterirdischen Bachlaufes","résurgence d'une rivière souterraine",2]
["Hydrogeology","Surface_Water_PT",12501004,"Versickerungsstelle eines Baches","perte d´un cours d´eau",2]
["Hydrogeology","Surface_Water_PT",12501005,"Steilstufe in Bachrinne, Wasserfall","rapide d'un cours d'eau, cascade",2]
["Hydrogeology","Surface_Water_PT",12501006,"Grundwasseraufstoss","résurgence des eaux souterraines",2]
["Local Additional Informations","Artificial_Surface_Modifications_PLG",10401001,"künstlich verändertes Gelände","terrain modelé artificiellement",2]
["Local Additional Informations","Artificial_Surface_Modifications_PLG",10401002,"künstliche Ablagerung, undifferenziert","dépôts artificiels, indifférenciés",2]
["Local Additional Informations","Artificial_Surface_Modifications_PLG",10401005,"Deponie","décharge",2]
["Local Additional Informations","Fossils_PT",12901001,"Fossilfundstelle","gisement fossilifère",2]
["Local Additional Informations","Indication_of_Resources_PT",13201004,"Tasche, Karsttasche, Kluft, mit Füllung von Siderolithikum","poche, poche karstique, fissure, remplie de matériel sidérolithique",2]
["Local Additional Informations","Indication_of_Resources_PT",13201005,"Fundstelle von vulkanischem Tuffit","gisement de tuffite volcanique",2]
["Local Additional Informations","Indication_of_Resources_PT",13201006,"Fundstelle vulkanischer Auswürflinge (Tephra)","gisement de projections volcaniques (tephra)",2]
["Local Additional Informations","Indication_of_Resources_PT",13201007,"Fundstelle von Ries-Auswürflingen","gisement de projections du Ries",2]
["Local Additional Informations","Mineralised_Zone_L",13301001,"Vererzungszone","zone minéralisée",2]
["Local Additional Informations","Sedimentary_Structures_PT",13401001,"Sedimentstrukturen","structures sédimentaires",2]
["Local Additional Informations","Sedimentary_Structures_PT",13401003,"Erosions- oder Omissionsfläche, Hartgrund, Kondensationshorizont","surface d´érosion ou lacune stratigraphique, surface durcie, niveau de condensation",2]
["Local Additional Informations","Type_Localities_PT",13501001,"geologisch relevanter Aufschluss","affleurement géologique important",2]
["Measurements and Spatial Orientation","Folds_PT",13601001,"Orientierung der Faltenachse","orientation d'un axe de pli",2]
["Measurements and Spatial Orientation","Folds_PT",13601002,"Orientierung der Scheitellinie","orientation d'une ligne de crête",2]
["Measurements and Spatial Orientation","Folds_PT",13601003,"Orientierung der Muldenlinie","orientation d'une ligne de creux",2]
["Measurements and Spatial Orientation","Lineation_PT",13701001,"Orientierung der Intersektionslineation","orientation de la linéation d´intersection",2]
["Measurements and Spatial Orientation","Lineation_PT",13701002,"Orientierung der Streckungslineation","orientation de la linéation d'étirement",2]
["Measurements and Spatial Orientation","Lineation_PT",13701004,"Orientierung von Gletscherschliffen","orientation des stries glaciaires",2]
["Measurements and Spatial Orientation","Planar_Structures_PT",13801002,"Orientierung eines Ganges","orientation d'un filon",2]
["Measurements and Spatial Orientation","Planar_Structures_PT",13801003,"Orientierung einer Bruchfläche","orientation d'un plan de faille",2]
["Rock Bodies","Unconsolidated_Deposits_PT",14401002,"Schwarm erratischer Blöcke","accumulation de blocs erratiques",2]
["Rock Bodies","Unconsolidated_Deposits_PT",14401006,"Sturzblock","bloc éboulé",2]
["Tectonics","Deformation_Structures_L",14701001,"Faltenscharnier","charnière de pli",2]
["Tectonics","Deformation_Structures_PLG",14801001,"Kluftzone","zone diaclasée",2]
["Tectonics","Deformation_Structures_PLG",14801002,"tektonisierte Zone","zone tectonisée",2]
["Tectonics","Deformation_Structures_PT",14601004,"Orientierung der Faltenachsenfläche","orientation de la surface axiale d'un pli",2]
["Tectonics","Deformation_Structures_PT",14601006,"Darstellung der Spur einer Achsenfläche","représentation de la trace d'une surface axiale",2]
["Tectonics","Deformation_Structures_PT",14601007,"Chevron-Falte, Kink Fold","plis en chevron, Kink Fold",2]
["Tectonics","Tectonic_Boundaries_L",14901005,"Aufschiebung","faille inverse",2]
["Tectonics","Tectonic_Boundaries_L",14901006,"Blattverschiebung","décrochement",2]
["Tectonics","Tectonic_Boundaries_L",14901007,"Komplexe Störung","accident tectonique complexe",2]
["Tectonics","Tectonic_Boundaries_L",14901008,"Störung i. Allg.","accident tectonique en général",2]
["Anthropogenic Features","Archaeology_L",10201001,"Verkehrsweg","voie de communication",3]
["Anthropogenic Features","Archaeology_L",10201002,"Hohlweg","chemin creux",3]
["Anthropogenic Features","Archaeology_L",10201003,"künstlicher Graben, Befestigungsgraben","fossé artificiel, fossé de fortification",3]
["Anthropogenic Features","Archaeology_L",10201004,"künstlicher Erdwall","levée de terre artificielle",3]
["Anthropogenic Features","Archaeology_L",10201005,"Wasserleitung","aqueduc",3]
["Anthropogenic Features","Archaeology_L",10201006,"Steinreihe","alignement mégalithique",3]
["Anthropogenic Features","Archaeology_L",10201007,"Schützengraben","tranchée",3]
["Anthropogenic Features","Archaeology_PLG",10301001,"Castrum","castrum",3]
["Anthropogenic Features","Archaeology_PLG",10301002,"Refugium, Höhensiedlung, Erdwerk","refugium, oppidum, fortification",3]
["Anthropogenic Features","Archaeology_PT",10101001,"archäologische Fundstelle, Anlage, Siedlungsreste","site archéologique, station, vestiges d'établissement",3]
["Anthropogenic Features","Archaeology_PT",10101002,"Höhlensiedlung, Abri","grotte, abri sous roche",3]
["Anthropogenic Features","Archaeology_PT",10101003,"Pfahlbauten","palafitte",3]
["Anthropogenic Features","Archaeology_PT",10101004,"Burgstelle, Burghügel, Wachtturm","motte, emplacement d´un ancien château, d´une fortification, d'un château-fort",3]
["Anthropogenic Features","Archaeology_PT",10101005,"Gräber, Gräberfeld","tombe, site mortuaire",3]
["Anthropogenic Features","Archaeology_PT",10101006,"Steinplattengrab","sépulture",3]
["Anthropogenic Features","Archaeology_PT",10101007,"Grabhügel, Dolmengrab","tumulus, dolmen funéraire",3]
["Anthropogenic Features","Archaeology_PT",10101008,"Kultstein","mégalithe",3]
["Anthropogenic Features","Archaeology_PT",10101009,"Kalkofen","four à chaux",3]
["Anthropogenic Features","Archaeology_PT",10101010,"Felsenkeller","cave dans la roche",3]
["Anthropogenic Features","Archaeology_PT",10101011,"Schlackenhalde","crassier",3]
["Anthropogenic Features","Archaeology_PT",10101012,"Glashütte","verrerie",3]
["Anthropogenic Features","Archaeology_PT",10101013,"Schmelzofen","four à fer",3]
["Anthropogenic Features","Archaeology_PT",10101014,"Schalenstein","pierre à crupules",3]
["Anthropogenic Features","Archaeology_PT",10101015,"Abbaustelle","exploitation",3]
["Anthropogenic Features","Boreholes_PT",10501001,"Bohrung","forage",3]
["Anthropogenic Features","Boreholes_PT",10501002,"Sondierschlitz","fouille ou tranchée de reconnaissance",3]
["Anthropogenic Features","Boreholes_PT",10501003,"Handsondierung","sondage à la tarière",3]
["Anthropogenic Features","Boreholes_PT",10501004,"Rammsondierung","sondage au pénétromètre",3]
["Anthropogenic Features","Boreholes_PT",10501005,"Rammkernsondierung","sondage par carottier battu",3]
["Anthropogenic Features","Exploitation_Geomaterials_L",10701001,"Abbaufront","front d'exploitation",3]
["Anthropogenic Features","Exploitation_Geomaterials_L",10701002,"Bergwerksstollen","galerie de mine",3]
["Anthropogenic Features","Exploitation_Geomaterials_PLG",10801001,"Steinbruch","carrière",3]
["Anthropogenic Features","Exploitation_Geomaterials_PLG",10801002,"Grube (Lockergesteinsabbau)","exploitation de matériaux meubles",3]
["Anthropogenic Features","Exploitation_Geomaterials_PT",10601001,"Bergwerk, Untertageabbau","mine, exploitation souterraine",3]
["Anthropogenic Features","Exploitation_Geomaterials_PT",10601002,"Stolleneingang","entrée de galerie",3]
["Anthropogenic Features","Exploitation_Geomaterials_PT",10601003,"Schacht","puits de mine",3]
["Anthropogenic Features","Exploitation_Geomaterials_PT",10601004,"Pinge (dolinenartiger Stolleneinbruch)","fontis (effondrement de surface lié à des travaux souterrains)",3]
["Anthropogenic Features","Exploitation_Geomaterials_PT",10601005,"Schürflöcher","trace d´exploitation en surface",3]
["Anthropogenic Features","Exploitation_Geomaterials_PT",10601006,"ausgeräumte Bohnerztaschen","poche sidérolithique vidée",3]
["Geomorphology","Alluvial_and_Lacustrine_Structures_L",10901001,"Strandwall","cordon littoral",3]
["Geomorphology","Erosional_Structures_L",11101003,"Schichtstufenkante","escarpement en tête de banc",3]
["Geomorphology","Erosional_Structures_PT",11001001,"Erdpyramide","demoiselle coiffée",3]
["Geomorphology","Glacial_and_Periglacial_Structures_L",11301005,"Schliffgrenze","limite supérieure de l'érosion glaciaire (trimline)",3]
["Geomorphology","Glacial_Structures_PT",11201001,"glazialtektonische Deformation","déformation glaciotectonique",3]
["Geomorphology","Karstic_Structures_PT",11901002,"Höhle, Balme","grotte, baume",3]
["Hydrogeology","Construction_L",12201001,"Wasserfassungsstollen","galerie de captage d´eau",3]
["Hydrogeology","Construction_L",12201002,"Künstlicher Gewässerlauf","écoulement artificiel",3]
["Hydrogeology","Construction_PT",12101001,"Grundwasserfassung","captage dans la nappe phréatique",3]
["Hydrogeology","Construction_PT",12101002,"Zisterne","citerne",3]
["Hydrogeology","Construction_PT",12101003,"laufender Brunnen (in wasserarmem Gebiet)","fontaine (en région sèche)",3]
["Hydrogeology","Construction_PT",12101004,"Sodbrunnen","puits",3]
["Hydrogeology","Construction_PT",12101005,"Versickerungsschacht","puits d´infiltration",3]
["Hydrogeology","Construction_PT",12101006,"Limnigraph","limnigraphe",3]
["Hydrogeology","Construction_PT",12101007,"Piezometer","piézomètre",3]
["Hydrogeology","Construction_PT",12101008,"Pumpwerk mit See- bzw. Flusswasserfassung","station de pompage avec captage en lac ou rivière",3]
["Hydrogeology","Construction_PT",12101009,"Pumpwerk ohne Wasserfassung","station de pompage sans captage d'eau",3]
["Hydrogeology","Subsurface_Water_L",12401001,"unterirdischer Gewässerlauf","écoulement souterrain",3]
["Hydrogeology","Surface_Water_PT",12501001,"Quelle","source",3]
["Local Additional Informations","Anomalies_PT",12801001,"gemessene Anomalie","anomalie mesurée",3]
["Local Additional Informations","Anomalies_PT",12801002,"Fulgurit","fulgurite",3]
["Local Additional Informations","Artificial_Surface_Modifications_PLG",10401006,"Halde","terril",3]
["Local Additional Informations","Indication_of_Resources_PT",13201001,"Mineralfundstelle","gisement de minéraux",3]
["Local Additional Informations","Indication_of_Resources_PT",13201002,"Gasquelle","source de gaz naturel",3]
["Local Additional Informations","Indication_of_Resources_PT",13201003,"Anzeichen auf Öl","indices de pétrole",3]
["Local Additional Informations","Indication_of_Resources_PT",13201008,"Asphalt, vereinzeltes Vorkommen","asphalte, gisement isolé",3]
["Local Additional Informations","Indication_of_Resources_PT",13201009,"Meteoritfundstelle","gisement de météorite",3]
["Local Additional Informations","Sedimentary_Structures_PT",13401002,"Riffstrukturen","structures récifales",3]
["Local Additional Informations","Sedimentary_Structures_PT",13401004,"stratigraphische Lage (Polarität) einer Schichtserie","position stratigraphique (polarité) d´une couche sédimentaire",3]
["Local Additional Informations","Sedimentary_Structures_PT",13401005,"Winkeldiskordanz","discordance angulaire",3]
["Measurements and Spatial Orientation","Lineation_PT",13701003,"Orientierung von Rutschharnischen","orientation des tectoglyphes",3]
["Measurements Spatial Orientation","Planar_Structures_PT",13801006,"Schüttungsrichtung","direction de transport sédimentaire",3]
["Parameter and Modelling","Contour_Lines_Bedrock_L",13901001,"Isohypse","isohypse",3]
["Parameter and Modelling","Contour_Lines_Hydro_L",14001001,"Isohypse des Grundwasserspiegels","isohypse de la surface piézométrique",3]
["Parameter and Modelling","Modelled_Water_Table_PT",14101001,"Grundwasserfliessrichtung","direction d'écoulement",3]
["Parameter and Modelling","Modelled_Water_Table_PT",14101002,"mittlere Höhe des Grundwasserspiegels","niveau moyen de la nappe phréatique",3]
["Parameter and Modelling","Slope_Bedrock_PT",14201001,"Neigungsrichtung","direction de plongement",3]
["Rock Bodies","Unconsolidated_Deposits_PT",14401001,"erratischer Block","bloc erratique",3]
["Rock Bodies","Unconsolidated_Deposits_PT",14401003,"anthropogene Ansammlung von erratischen Blöcken","amas anthropique de blocs erratiques",3]
["Rock Bodies","Unconsolidated_Deposits_PT",14401004,"Wanderblock","bloc laboureur",3]
["Rock Bodies","Unconsolidated_Deposits_PT",14401005,"Geschiebe","cailloutis glaciaire",3]
["Rock Bodies","Unconsolidated_Deposits_PT",14401007,"Lesesteinhaufen","dépôt d'épierrage",3]
["Rock Bodies","Unconsolidated_Deposits_PT",14401008,"Verwitterungsrückstände (Gerölle und/oder Konkretionen)","éléments résiduels (galets et/ou rognons)",3]
["Tectonics","Deformation_Structures_PT",14601001,"punktuell beobachtete tektonische Brekzie","brèche tectonique observée ponctuellement",3]
["Tectonics","Deformation_Structures_PT",14601002,"ausgeprägte Klüftung","diaclases bien marquées",3]
["Tectonics","Deformation_Structures_PT",14601003,"tektonische Diskordanz","discordance tectonique",3]
["Tectonics","Deformation_Structures_PT",14601005,"Fältelung","plissotement (plis)",3]
["Hydrogeology","Surface_Water_L",12601002,"Bachlauf","ruisseau",5]